Fortinet

Configuración Minicom

pu port /dev/ttyUSB0 pu baudrate 9600 pu bits 8 pu parity N pu stopbits 1 pu hasdcd No pu rtscts No pu xonxoff No

Acceder sin password de admin

Prendemos el equipo y vamos a tener 30 segundos para logearnos por la terminal de consola. Luego de esos 30 segundos la información de login va a ser inválida.

El usuario es: maintainer

La contraseña es bcpb + número de serie.

Ejemplo: bcpbFGT60C3G10016011

Comandos

Equivalencias con CISCO

show

Show global or vdom config

sh system interface

Equivalent to show run interface

diagnose hardware deviceinfo nic

Equivalent to show interface

get system status

show version information

sh firewall policy 6

show firewall rule numer 6

sh router policy

Show Policy Routing rules

diagnose system session list

Show the excisting translations

diagnose system session clear

Clears all xlate/translations

diagnose ip arp list

Shows the arp table of connected hosts

get router info routing-table all

Equivalent to ‘show ip route’

diagnose system top

Show System Processes running with PIDs

diagnose system kill 9 <id>

Kill the specific PID

Referencia : https://routing-bits.com/2008/10/09/fortigate-commands/

Forti OS

Reiniciar valores de fabrica

exec factoryreset

Ver configuración de interfaces

show system interface ?

Sniff de paquetes SNMP

Útil para verificar si el ruteo funciona correctamente

diag sniffer packet any icmp

Ver tablas de ruteo

get router info routing-table details

Diánosticar VPN

get vpn ike gateway

get vpn ipsec tunnel details

diagnose vpn tunnel list

diagnose vpn ipsec status

Equipos